**Modeling Electrical Conductivity and Transfer Characteristics of n- and p-Type Graphene/MoS2 Hetero-structures**

Van-Khoe Nguyen1,2,3, Shih-Yen Lin1, Yia-Chung Chang1

1Research Center for Applied Sciences, Academia Sinica, Taipei 115, Taiwan

2Department of Physics, National Central University, Jhongli 320, Taiwan

3Molecular Science and Technology Program, Taiwan International Graduate Program, Academia Sinica, Taipei 115, Taiwan

Graphene being a gapless semimetal intrinsically has very high mobility but rather low on/off ratio. MoS2 is an indirect semiconductor with a band gap of ~1.2 eV, and it becomes a direct semiconductor with a bigger band gap of ~1.9 eV when being exfoliated as a monolayer two-dimensional material. MoS2 has much lower mobility but can reach rather higher on/off ratio than graphene. Therefore, they are expected to complement each other in theirhetero-structures with high mobility and high on/off ratio. Here we present a model calculation of electrical conductivity and transfer characteristics of n- and p-type graphene/MoS2 hetero-structures for different numbers of MoS2 monolayers and, accordingly, of different types and values of the band gap, at various temperatures under a large range of gate voltages. Our model takes account of electron-phonon interactions and many-body effects. Our calculated results for I-V characteristics and carrier densities as functions of gate voltages agree rather well with the available experimental data with the use of a few physical parameters (including the band offset, defect scattering rates, and fraction of the applied gate voltage in the active region), which all fall into a reasonable range. Therefore, our approach can also be applicable to graphene/transition metal dichalcogenides (TMDs) hetero-structures.